******************************************************************************
**                                                                          **
**    FANUC Program Transfer Tool         (A08B-9510-J515) Edition 16.0     **
**                                                                          **
**        Copyright(c) 2007- FANUC CORPORATION  All rights reserved.        **
**                                                                          **
******************************************************************************
------------------------------------------------------------------------------

This document provides the information about "FANUC Program Transfer Tool".
Please read the following information before using the software.
If the contents of this file are different from the manual(B-64344EN) then use
the information of this file.

--------------------------------------------------------------------------
[1] Environment
[2] Installation
[3] Update history
--------------------------------------------------------------------------

==============================================================================
[1] Environment
==============================================================================
1.1. Supported OS
    Program Transfer Tool supports the following OS.
      - Windows 10 Pro                (32/64bit OS)
      - Windows 8 Pro                 (32/64bit OS)
      - Windows 7 Professional SP1    (32/64bit OS)
      - Windows Vista Business SP2    (32bit OS)
      - Windows XP Professional SP3   (32bit OS)

    Display : 1024x768 or higher resolution
    Vacant capacity of hard disk : 30Mbytes or more

1.2. Program Transfer Tool can be used with the following CNC:
      - Series 30i/31i/32i-MODEL A/B
      - Series 35i-MODEL B
      - Power Motion i-A
      - Series 0i-MODEL B/C/D/F
      - Series 16i/18i/21i-MODEL A/B
      - Series 20i-MODEL B
      - Power Mate i-MODEL D/H

   The Ethernet or Data Server function is required to CNC.
   The PCMCIA LAN card is not supported.

==============================================================================
[2] Installation
==============================================================================
2.1. Procedure of installation
     - The administrator privilege is required to installing.
     - Silent installation is not supported.

    (1) Set CD-ROM in CD-ROM drive.
    (2) The installer will be started automatically.
    
    Follow the instructions which are displayed in PC.

2.2 Serial No.
    After the installing, the serial number is required on the setting dialog.
    The serial number paper is included in the CD-ROM case.

2.3 Procedure of update
    - It is possible to update from old specification, A08B-9510-J513 or
      A08B-9510-J514, to the new specification, A08B-9510-J515.
    - The following updating procedure is different:
        (a) Version 1.0 -> Version 2.0
        (b) Version 2.0 -> Version 3.0 or later
      Please refer to the manual for the detail.

==============================================================================
[3] Update history
==============================================================================

   Version 16.0 (June, 2019)
        - The download speed to the program storage file (FANUCPRG.BIN) stored
          in the memory card of CNC is improved.
        - Even if the Program Folder Screen is displayed on the CNC while 
          downloading or uploading multiple text files to or from the CNC 
          memory card, the transfer have been supported.

   Version 15.0 (Nov.,2018)
        - Program storage file (named "FANUCPRG.BIN") in the memory card of CNC
          has been supported.
        - The number of path(head) supported by the tool has been expanded to 
          15.

   Version 14.0 It is a missing number.

   Version 13.0 (May,2018)
        - Communication may be terminated when operation is not performed for
          a certain period of time after connecting this tool and CNC.
          This phenomenon may occur in Windows Vista or later OS.
          It has improved so that this phenomenon does not occur.

   Version 12.0 (Mar.,2017)
        - Memory card of CNC is supported.

   Version 11.0 It is a missing number.

   Version 10.0 (Nov.,2014)
        - Series 0i-MODEL F has been supported.
        - Windows 10 Pro(32bit/64bit OS) has been supported.

   Version 9.0 (June,2014)
        - License and specification has been changed.
          License
            The single computer license has been changed to the site license.
            Please refer to the "LICENSE AGREEMENT" for details.

          New specification
            A08B-9510-J515
          Old specifications are abolished.
            A08B-9510-J513
            A08B-9510-J514

   Version 8.0 (Aug.,2011)
        - Power Motion i-A has been supported.
        - Windows 8 Pro(32bit/64bit OS) has been supported.

   Version 7.0 (Feb.,2011)
        - Windows 7 Professional(64bit OS) has been supported.

   Version 6.0 (Oct.,2010)
        - Series 30i/31i/32i-MODEL B, Series 35i-MODEL B has been supported.

   Version 5.1 (May,2010)
        - The following error may be occurred at downloading.
            "Retry because the buffer is full."
          This problem is corrected.

   Version 5.0 (Apr.,2010)
        - Windows 7 Professional(32bit OS) has been supported.

   Version 4.0 (Sep.,2008)
        - Transferring tool management data of Series 30i/31i/32i-MODEL A has
          been supported.

   Version 3.0 (May.,2008)
        - Series 0i-MODEL D has been supported.
        - Simplified Chinese has been supported.

   Version 2.0 (Dec.26,2007)
        - Windows Vista Business(32bit OS) has been supported.
        - Upgrade CD is added.

   Version 1.0 (Oct.03,2007)
        - New creation

**  Microsoft, Windows, Windows XP, Windows Vista, Windows 7, Windows 8, and
    Windows 10 are trademarks or registered trademarks of Microsoft Corporation.
**  Other product names mentioned are trademarks or registered trademarks
    of their respective companies.
